Doc 5d - Price Schedule

Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Tender Ref: OCT-23-128**

Please mention your bid / quote on this form along with your sign and stamp on each page or in the same manner on your letter head.

Delivery Location: Project area of District Shaheed Benazirabad, Sindh, Pakistan.

Lot No. 04 Construction of Permanent Hand Washing Stations in Health Facilities (Total 09 Sites)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Sr. No.** | **Item Name** | **Unit** | **Quantity** | **Unit price of 1 item inclusive of taxes, packing, loading/ unloading, Transportation to Delivery Location of District Shaheed Benazirabad, Sindh**  **(To be filled in PKR by the bidder)** | **Total price inclusive of taxes, packing, loading/ unloading, Transportation to Delivery Location of District Shaheed Benazirabad, Sindh**  **(To be filled in PKR by the bidder)** | **Delivery Time in Days after PO/Supplies Contract** |
| 1 | Dismentalling work | Job | 1.00 |  |  |  |
| 2 | Excavation in foundation of building, bridges etc. complete in ordinary soil with Backfill | Cft | 20.50 |  |  |  |
| 3 | Plain Cement Concrete including placing, compacting, finishing & curing (Ratio 1:4:8) | Cft | 11.63 |  |  |  |
| 4 | Provide & laying of Plain Cement Concrete 1:2:4, including surface finishing, curing complete finsh work | Cft | 15.00 |  |  |  |
| 5 | Filling, watering and ramming earth under floor with earth excavated from outside lead upto 30m | Cft | 45.00 |  |  |  |
| 6 | Provide, lay, water & ram 4" thick clean coarse sand under floor / brick paving, complete | Cft | 15.00 |  |  |  |
| 7 | 1st class brick work in Foundation, Super structure in Cement, sand mortar 1:6 | Cft | 107.63 |  |  |  |
| 8 | RCC in roof slab, beam, column & other structural members, insitu or precast. Type C (1:2:4) | Cft | 4.00 |  |  |  |
| 9 | Supply & fabricate M.S. reinforcement for cement concrete, (Hot rolled deformed bars Grade 40) | KG | 13.34 |  |  |  |
| 10 | 1/2" thick cement plaster 1:4 on walls, inner, outer sides, including making edges, corners, and curing, etc., complete in all aspects. | Sft | 144.00 |  |  |  |
| 11 | Providing and Fixing Ceramic Tiles on walls and floors of approved quality, on wall up to 5 feet height, including, bonds, cutting, fixing etc., complete in all aspects.. | Sft | 101.25 |  |  |  |
| 12 | Painting new surface ( weather shield of approved quality) | Sft | 98.00 |  |  |  |
| 13 | P/F of 3 mm (3 ply) fiber shed with the frame of 2" MS pipe of 16 gauge having distance 2'x2' fitting on 3" dia MS round pipe 4mm thick including 3 coats enamel paint and grounding with concrete 1:2:4 as directed by engineer. (10' height from Finish Floor Level) | Sft | 36.00 |  |  |  |
| 14 | Providing and Fixing glazed earthen ware wash hand basin (WHB) white in color of Porta or Bright, complete, size 56x40 cm (22"x16"), including pedestal, bracket set, Side Pillar Cook Water Tap, waste coupling, 1-1/4'' Ф strainers, 1-1/4'' Ф drain pipe, soap dish, complete in all respects: | No | 2 |  |  |  |
| 15 | Providing, laying cutting, jointing, upvc pipeline 3/4" dia in walls/trenches with pipes of approved quality for cold/hot water supply systems including the cost of accessories e.g. Socket, Union, Elbow, Tee, Bend, valves etc. Work also includes digging/burying up to 1 feet depth in ground and in walls in all types of soil, soft & hard. Master or equivalent. | Rft | 100 |  |  |  |
| 16 | Supply and installation of UPVC PIPE of 3" dia with all connections, fixture including all accessories (Socket, elbows, bends, Tee, etc.) to dispose off wastewater up to manhole or designated site by site engineer. Including digging/burying of PVC Pipe up to 1 feet depth in all kind of the material. Dadex, Master or equivalent-Class. | Rft | 40 |  |  |  |
| 17 | Providing and fixing of liquid soap dispenser.(filled) | No | 2 |  |  |  |
| 18 | Providing and fixing of mirror set along with soap tray, plastic tissue holder box, toilet roll holder etc. | No | 2 |  |  |  |
| 19 | Visibility plate 15"X12", 20-22 SWG, stainless steel, holes for nails Complete Write up as per instruction of client, including fixing work complete in all aspects | No | 1 |  |  |  |
| 20 | Pre-Cast RCC slabs having size bracing thickness 2'', centre thickness 3/4'' Complete inclduing Girders for support & grouting above slabs | Sft | 16 |  |  |  |
| **TOTAL AMOUNT for 01 Hand Washing Station** | | | | |  | |
| **TOTAL AMOUNT for 09 Hand Washing Stations** | | | | |  | |

Grand Total Amount in words: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Name of Bidder Signature & Stamp of Bidder Date

Contact Number Email Address

Office Address