Doc 5b - Price Schedule

Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Tender Ref: OCT-23-128**

Please mention your bid / quote on this form along with your sign and stamp on each page or in the same manner on your letter head.

Delivery Location: Project area of District Shaheed Benazirabad, Sindh, Pakistan.

Lot No. 02 Repair & Renovation Work of Critical Infrastructure (Total 09 Sites)

1. ***REPAIR AND RENOVATION MINOR WORK OF BHU MARI JALBANI DISTRICT SHAHEED BENAZIR ABAD, SINDH PAKISTAN***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Sr. No.** | **Item Name** | **Unit** | **Quantity** | **Unit price of 1 item inclusive of taxes, packing, loading/ unloading, Transportation to Delivery Location of District Shaheed Benazirabad, Sindh**  **(To be filled in PKR by the bidder)** | **Total price inclusive of taxes, packing, loading/ unloading, Transportation to Delivery Location of District Shaheed Benazirabad, Sindh**  **(To be filled in PKR by the bidder)** | **Delivery Time in Days after PO/Supplies Contract** |
| **A** | **Civil Works** |  |  |  |  |  |
| 1 | Dismantling cement concrete/ Brick work etc | Cft | 31.50 |  |  |  |
| 2 | Plain Cement Concrete including placing, compacting, finishing & curing (Ratio 1:4:8) | Cft | 2.51 |  |  |  |
| 3 | Pacca brick work in cement mortar in 1:6 ratio in Ground Floor as directed by Engineer In charge | Cft | 27.00 |  |  |  |
| 4 | Reinforced cement concrete work including all labour and material except the cost of steel reinforcement and its labour for bending and binding which will be paid separately. This rate also includes all kinds of forms moulds, lifting shuttering curing rendering and finishing the exposed surface (including screening and washing of shingle. (a)R.C work in roof slab, beams, columns rafts, lintels and other structural members laid in situ or precast laid in position complete in all respect.(I) Ratio 1:2:4 | Cft | 126.53 |  |  |  |
| 5 | Fabrication of mild steel reinforcement for cement concrete i/c cutting & bending and laying in position, making joints and fastenings including cost of binding wire(also includes removal of rust from bars) | KG | 281.31 |  |  |  |
| 6 | Repair of Doors & Windows including (Panels replacement, Hinges, Bolts, Locks etc) | Nos | 5.00 |  |  |  |
| 7 | P/F GI Frame chowkhat Size 7"\*2" for Door using 20 gauge G.I Sheet I/C welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage, tools and plants using in making and fixing etc. complete. | Rft | 35.00 |  |  |  |
| 8 | Plain Cement Concrete including placing, compacting, finishing & curing (Ratio 1:2:4) | Cft | 13.20 |  |  |  |
| 9 | Removing cement or lime plaster | Sft | 155.00 |  |  |  |
| 10 | Applying Floating coat of cement 1/32" thick | Sft | 155.00 |  |  |  |
| 11 | Cement plaster 1:4 up to 20ft Heights & 1/2'' thick etc. complete | Sft | 155.00 |  |  |  |
| 12 | Distempering three coat include scraping, Filling & Making surface smooth etc. complete as directed by engineer in charge. | Sft | 3970.74 |  |  |  |
| 13 | Preparing The Surface & painting with weather coat i/c rubbing the surface with rubbing brick / sand paper, filling the voids with chalk plaster of Paris & then painting weather coat of approved make. | Sft | 6949.50 |  |  |  |
| 14 | Painting of surface any type doors & window etc. complete in three coat. | Sft | 1159.00 |  |  |  |
| 15 | Providing and fixing in position doors, windows and ventilators of 1st class deodar wood frames and 1-1/2" thick teak wood ply shutters of 2nd class deodar wood skeleton (Solid) styles and rails core of partial wood and teak ply wood (3-ply) on both sides i/c holds fasts, hinges, iron tower bolts, handles and cleats with cord etc complete | Sft | 35.00 |  |  |  |
| 16 | Cleaning of Toilets & Sewerage Lines | Job | 1.00 |  |  |  |
| 17 | Roof cleaning two coat cementation German acrylic chemical cracke filling and bandage laying of canvas cloth 4 Onz entire roof then apply two coat cementation German acrylic chemical, finally apply one coat Everseal. | Sft | 3024.00 |  |  |  |
| **B** | **PLUMBING WORK** |  |  |  |  |  |
| 1 | P/Fixing orise type white or colour glazed earthen ware WC Pan including P Trap & Complete with all other fixtures as directed by engineer incharge | No | 2 |  |  |  |
| 2 | Supplying/Fixing long bib cock of superior quality with c.p head 1/2' dia. (master, sonex,Porta brands). | No | 2 |  |  |  |
| 3 | Providing and fixing 1/2" and 3/4" dia UPVC pipe make Pak Arab include cutting, fitting including all fixtures etc complete as directed by engineer incharge. | Rft | 200 |  |  |  |
| 4 | P/Laying of RCC pipe 6" dia B class and digging trenches to required depth in fixing position including cutting, fixing, jointing & backfilling etc | Rft | 220 |  |  |  |
| **C** | **Sign Board / Plaque** |  |  |  |  |  |
| 1 | Supply and installation of Sign Board / Branding sheet with organisation / Donors logos complete as per approved Design or as instructed by Engineer Incharge. | Job | 1 |  |  |  |
| **Sub-Total (I)** | | | | |  | |

1. ***REPAIR AND RENOVATION MINOR WORK OF BHU PLUS JALALANI (PPHI) DISTRICT***

***SHAHEED BENAZIR ABAD, SINDH PAKISTAN***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Sr. No.** | **Item Name** | **Unit** | **Quantity** | **Unit price of 1 item inclusive of taxes, packing, loading/ unloading, Transportation to Delivery Location of District Shaheed Benazirabad, Sindh**  **(To be filled in PKR by the bidder)** | **Total price inclusive of taxes, packing, loading/ unloading, Transportation to Delivery Location of District Shaheed Benazirabad, Sindh**  **(To be filled in PKR by the bidder)** | **Delivery Time in Days after PO/Supplies Contract**  **(To be filled in PKR by the bidder)** |
| **A** | **Civil Works** |  |  |  |  |  |
| 1 | Excavation in foundation of building, bridges, footpath, roads and other structure include dag, belling dressing refilling around structure with excavated earth watering and ramming lead up to 5ft etc. complete as directed by engineer in charge | Cft | 242.50 |  |  |  |
| 2 | Pacca brick work in cement mortar in 1:6 ratio in Ground Floor as directed by Engineer In charge | Cft | 240.69 |  |  |  |
| 3 | Reinforced cement concrete work including all labour and material except the cost of steel reinforcement and its labour for bending and binding which will be paid separately. This rate also includes all kinds of forms moulds, lifting shuttering curing rendering and finishing the exposed surface (including screening and washing of shingle. (a)R.C work in roof slab, beams, columns rafts, lintels and other structural members laid in situ or precast laid in position complete in all respect.(I) Ratio 1:2:4 | Cft | 7.81 |  |  |  |
| 4 | Fabrication of mild steel reinforcement for cement concrete i/c cutting & bending and laying in position, making joints and fastenings including cost of binding wire(also includes removal of rust from bars) | KG | 26.05 |  |  |  |
| 5 | Repair of Doors & Windows including (Panels replacement, Hinges, Bolts, Locks etc) | Nos | 2.00 |  |  |  |
| 6 | Removing cement or lime plaster | Sft | 200.00 |  |  |  |
| 7 | Applying Floating coat of cement 1/32" thick | Sft | 200.00 |  |  |  |
| 8 | Cement plaster 1:4 up to 20ft Heights & 1/2'' thick etc. complete | Sft | 589.00 |  |  |  |
| 9 | Distempering three coat include scraping, Filling & Making surface smooth etc. complete as directed by engineer in charge. | Sft | 8038.00 |  |  |  |
| 10 | Preparing The Surface & painting with weather coat i/c rubbing the surface with rubbing brick / sand paper, filling the voids with chalk plaster of Paris & then painting weather coat of approved make. | Sft | 8336.00 |  |  |  |
| 11 | Painting of surface any type doors & window etc. complete in three coat. | Sft | 1328.00 |  |  |  |
| 12 | laying floor of approved coloured glazed tiles 1/4" thick laid in white cement and pigment on a bed of 3/4" Thick cement motor 1:2 | Sft | 25.00 |  |  |  |
| 13 | Glazed tiles/dado/skirting 1/4" thick laid in pigment over 1:2 ratio cement sand motor 3/4" thick including finishing | Sft | 20.00 |  |  |  |
| 14 | Providing and fixing in position doors, windows and ventilators of 1st class deodar wood frames and 1-1/2" thick teak wood ply shutters of 2nd class deodar wood skeleton (Solid) styles and rails core of partial wood and teak ply wood (3-ply) on both sides i/c holds fasts, hinges, iron tower bolts, handles and cleats with cord etc complete | Sft | 36.00 |  |  |  |
| 15 | Roof cleaning two coat cementation German acrylic chemical cracke filling and bandage laying of canvas cloth 4 Onz entire roof then apply two coat cementation German acrylic chemical, finally apply one coat Everseal. | Sft | 2025.00 |  |  |  |
| **B** | **PLUMBING WORK** |  |  |  |  |  |
| 1 | P/Fixing Muslim Shower | No | 1 |  |  |  |
| 2 | Supplying/Fixing long bib cock of superior quality with c.p head 1/2' dia. (master, sonex,Porta brands). | No | 4 |  |  |  |
| 3 | Supplying & Fixing fibre glass tank of approved quality and design and wall thickness as specified I/c cost of nuts, bolts and fixing in plateform of cement concrete 1:3:6 and making connections for in-let, & out-let & over flow pipes etc. complete 350 gallons wall thickness 3.5mm | No | 1 |  |  |  |
| 4 | Providing and fixing 1/2" and 3/4" dia UPVC pipe make Pak Arab include cutting, fitting including all fixtures etc complete as directed by engineer incharge. | Rft | 100 |  |  |  |
| 5 | P/Laying of RCC pipe 6" dia B class and digging trenches to required depth in fixing position including cutting, fixing, jointing & backfilling etc | Rft | 50 |  |  |  |
| 6 | Providing, laying UPVC pressure pipes of Class 'B'( equivalent make) digging trenches to required depth, fixing in trench i/c cutting, fitting and jointing with all fixers with 'Z' joint with one rubber ring i/c testing with water to a head 61 meter or 200ft & backfilling complete | Rft | 150 |  |  |  |
| 7 | P/Laying precast RCC slab 2" thick include all cost of labour transportation with fixing of existing main hole etc. complete as directed by engineer incharge. | Sft | 20 |  |  |  |
| **C** | **Sign Board / Plaque** |  |  |  |  |  |
| 1 | Supply and installation of Sign Board / Branding sheet with organisation / Donors logos complete as per approved Design or as instructed by Engineer Incharge. | Job | 1 |  |  |  |
| **Sub-Total (II)** | | | | |  | |

1. ***REPAIR AND RENOVATION MINOR WORK OF GD JHOOJHAN DISTRICT SHAHEED BENAZIRABA, SIND PAKISTAN***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Sr. No.** | **Item Name** | **Unit** | **Quantity** | **Unit price of 1 item inclusive of taxes, packing, loading/ unloading, Transportation to Delivery Location of District Shaheed Benazirabad, Sindh**  **(To be filled in PKR by the bidder)** | **Total price inclusive of taxes, packing, loading/ unloading, Transportation to Delivery Location of District Shaheed Benazirabad, Sindh**  **(To be filled in PKR by the bidder)** | **Delivery Time in Days after PO/Supplies Contract**  **(To be filled in PKR by the bidder)** |
| **A** | **Civil Works** |  |  |  |  |  |
| 1 | Dismantling cement concrete/ Brick work etc | Cft | 820.00 |  |  |  |
| 2 | Pacca brick work in cement mortar in 1:6 ratio in Ground Floor as directed by Engineer In charge | Cft | 108.24 |  |  |  |
| 3 | Reinforced cement concrete work including all labour and material except the cost of steel reinforcement and its labour for bending and binding which will be paid separately. This rate also includes all kinds of forms moulds, lifting shuttering curing rendering and finishing the exposed surface (including screening and washing of shingle. (a)R.C work in roof slab, beams, columns rafts, lintels and other structural members laid in situ or precast laid in position complete in all respect.(I) Ratio 1:2:4 | Cft | 147.13 |  |  |  |
| 4 | Fabrication of mild steel reinforcement for cement concrete i/c cutting & bending and laying in position, making joints and fastenings including cost of binding wire(also includes removal of rust from bars) | KG | 490.64 |  |  |  |
| 5 | Removing cement or lime plaster | Sft | 2212.22 |  |  |  |
| 6 | Applying Floating coat of cement 1/32" thick | Sft | 2212.22 |  |  |  |
| 7 | Cement plaster 1:4 up to 20ft Heights & 1/2'' thick etc. complete | Sft | 2212.22 |  |  |  |
| 8 | Distempering three coat include scraping, Filling & Making surface smooth etc. complete as directed by engineer in charge. | Sft | 3520.06 |  |  |  |
| 9 | Preparing The Surface & painting with weather coat i/c rubbing the surface with rubbing brick / sand paper, filling the voids with chalk plaster of Paris & then painting weather coat of approved make. | Sft | 2871.16 |  |  |  |
| 10 | Painting of surface any type doors & window etc. complete in three coat. | Sft | 1481.60 |  |  |  |
| 11 | laying floor of approved coloured glazed tiles 1/4" thick laid in white cement and pigment on a bed of 3/4" Thick cement motor 1:2 | Sft | 50.00 |  |  |  |
| 12 | Glazed tiles/dado/skirting 1/4" thick laid in pigment over 1:2 ratio cement sand motor 3/4" thick including finishing | Sft | 10.00 |  |  |  |
| 13 | Providing and fixing in position doors, windows and ventilators of 1st class deodar wood frames and 1-1/2" thick teak wood ply shutters of 2nd class deodar wood skeleton (Solid) styles and rails core of partial wood and teak ply wood (3-ply) on both sides i/c holds fasts, hinges, iron tower bolts, handles and cleats with cord etc complete | Sft | 269.50 |  |  |  |
| 14 | Cleaning of manholes, Septic Tank, Bushes etc. | job | 1.00 |  |  |  |
| 15 | Cleaning of Latrine, Bushes etc. | job | 1.00 |  |  |  |
| 16 | Repair of Main Gate including welding, locks & increasing height etc complete | job | 1.00 |  |  |  |
| 17 | Roof cleaning two coat cementation German acrylic chemical cracke filling and bandage laying of canvas cloth 4 Onz entire roof then apply two coat cementation German acrylic chemical, finally apply one coat Everseal. | Sft | 283.35 |  |  |  |
| **B** | **PLUMBING WORK** |  |  |  |  |  |
| 1 | P/Fixing orise type white or colour glazed earthen ware WC Pan including P Trap & Complete with all other fixtures as directed by engineer incharge | No | 2 |  |  |  |
| 2 | Supplying/Fixing long bib cock of superior quality with c.p head 1/2' dia. (master, sonex,Porta brands). | No | 4 |  |  |  |
| 3 | Providing and fixing 1/2" and 3/4" dia UPVC pipe make Pak Arab include cutting, fitting including all fixtures etc complete as directed by engineer incharge. | Rft | 150 |  |  |  |
| 4 | P/Laying of RCC pipe 6" dia B class and digging trenches to required depth in fixing position including cutting, fixing, jointing & backfilling etc | Rft | 100 |  |  |  |
| 5 | Providing, laying UPVC pressure pipes of Class 'B'( equivalent make) digging trenches to required depth, fixing in trench i/c cutting, fitting and jointing with all fixers with 'Z' joint with one rubber ring i/c testing with water to a head 61 meter or 200ft & backfilling complete | Rft | 30 |  |  |  |
| 6 | P/Laying precast RCC slab 2" thick include all cost of labour transportation with fixing of existing main hole etc. complete as directed by engineer incharge. | Sft | 20 |  |  |  |
| 7 | Vent pipe with cowel | Job | 2 |  |  |  |
| **C** | **Sign Board / Plaque** |  |  |  |  |  |
| 1 | Supply and installation of Sign Board / Branding sheet with organisation / Donors logos complete as per approved Design or as instructed by Engineer Incharge. | Job | 1 |  |  |  |
| **Sub-Total (III)** | | | | |  | |

1. ***REPAIR AND RENOVATION MINOR WORK OF GD KHADAR DISTRICT SHAHEED BENAZIR ABAD, SINBD PAKISTAN***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Sr. No.** | **Item Name** | **Unit** | **Quantity** | **Unit price of 1 item inclusive of taxes, packing, loading/ unloading, Transportation to Delivery Location of District Shaheed Benazirabad, Sindh**  **(To be filled in PKR by the bidder)** | **Total price inclusive of taxes, packing, loading/ unloading, Transportation to Delivery Location of District Shaheed Benazirabad, Sindh**  **(To be filled in PKR by the bidder)** | **Delivery Time in Days after PO/Supplies Contract**  **(To be filled in PKR by the bidder)** |
| **A** | **Civil Works** |  |  |  |  |  |
| 1 | Excavation in foundation of building, bridges, footpath, roads and other structure include dag, belling dressing refilling around structure with excavated earth watering and ramming lead up to 5ft etc. complete as directed by engineer in charge | Cft | 246.00 |  |  |  |
| 2 | Dismantling cement concrete/ Brick work etc | Cft | 82.63 |  |  |  |
| 3 | Plain Cement Concrete including placing, compacting, finishing & curing (Ratio 1:4:8) | Cft | 150.00 |  |  |  |
| 4 | Pacca brick work in cement mortar in 1:6 ratio in Ground Floor as directed by Engineer In charge | Cft | 158.63 |  |  |  |
| 5 | Reinforced cement concrete work including all labour and material except the cost of steel reinforcement and its labour for bending and binding which will be paid separately. This rate also includes all kinds of forms moulds, lifting shuttering curing rendering and finishing the exposed surface (including screening and washing of shingle. (a)R.C work in roof slab, beams, columns rafts, lintels and other structural members laid in situ or precast laid in position complete in all respect.(I) Ratio 1:2:4 | Cft | 21.43 |  |  |  |
| 6 | Fabrication of mild steel reinforcement for cement concrete i/c cutting & bending and laying in position, making joints and fastenings including cost of binding wire(also includes removal of rust from bars) | KG | 71.47 |  |  |  |
| 7 | Plain Cement Concrete including placing, compacting, finishing & curing (Ratio 1:2:4) | Cft | 20.04 |  |  |  |
| 8 | Removing cement or lime plaster | Sft | 180.00 |  |  |  |
| 9 | Applying Floating coat of cement 1/32" thick | Sft | 180.00 |  |  |  |
| 10 | Cement plaster 1:4 up to 20ft Heights & 1/2'' thick etc. complete | Sft | 488.00 |  |  |  |
| 11 | Distempering three coat include scraping, Filling & Making surface smooth etc. complete as directed by engineer in charge. | Sft | 5010.50 |  |  |  |
| 12 | Preparing The Surface & painting with weather coat i/c rubbing the surface with rubbing brick / sand paper, filling the voids with chalk plaster of Paris & then painting weather coat of approved make. | Sft | 3834.50 |  |  |  |
| 13 | Painting of surface any type doors & window etc. complete in three coat. | Sft | 571.00 |  |  |  |
| 14 | Providing and fixing in position doors, windows and ventilators of 1st class deodar wood frames and 1-1/2" thick teak wood ply shutters of 2nd class deodar wood skeleton (Solid) styles and rails core of partial wood and teak ply wood (3-ply) on both sides i/c holds fasts, hinges, iron tower bolts, handles and cleats with cord etc complete | Sft | 17.50 |  |  |  |
| 15 | Installation of Wire gauze including all fixers as instructed by engineer incharge | Sft | 160.00 |  |  |  |
| 16 | Cleaning of manholes, Septic Tank etc. | job | 1.00 |  |  |  |
| 17 | Roof cleaning two coat cementation German acrylic chemical cracke filling and bandage laying of canvas cloth 4 Onz entire roof then apply two coat cementation German acrylic chemical, finally apply one coat Everseal. | Sft | 3024.00 |  |  |  |
| **B** | **PLUMBING WORK** |  |  |  |  |  |
| 1 | P/Fixing orise type white or colour glazed earthen ware WC Pan including P Trap & Complete with all other fixtures as directed by engineer incharge | No | 2 |  |  |  |
| 2 | P/Fixing 3 Gallon Flushing Cistern Complete with all fixtures as per instruction of Engineer incharge | No | 2 |  |  |  |
| 3 | P/Fixing 6"x2" x3" C.I floor trap of approved self cleaning design with a C.I screwed down gritting with or without a vent arm complete. | No | 2 |  |  |  |
| 4 | Supplying/Fixing long bib cock of superior quality with c.p head 1/2' dia. (master, sonex,Porta brands). | No | 3 |  |  |  |
| 5 | S/Fixing of concealed stop cock/Pillar of Superior quality with CP head 1/2" dia. | No | 3 |  |  |  |
| 6 | Supplying & Fixing fibre glass tank of approved quality and design and wall thickness as specified I/c cost of nuts, bolts and fixing in plateform of cement concrete 1:3:6 and making connections for in-let, & out-let & over flow pipes etc. complete 350 gallons wall thickness 3.5mm | No | 1 |  |  |  |
| 7 | Providing and fixing 1/2" and 3/4" dia UPVC pipe include cutting, fitting including all fixtures etc complete as directed by engineer incharge. | Rft | 200 |  |  |  |
| 8 | P/Laying of RCC pipe 6" dia B class and digging trenches to required depth in fixing position including cutting, fixing, jointing & backfilling etc | Rft | 40 |  |  |  |
| 9 | Providing, laying UPVC pressure pipes of Class 'B'( equivalent make) digging trenches to required depth, fixing in trench i/c cutting, fitting and jointing with all fixers with 'Z' joint with one rubber ring i/c testing with water to a head 61 meter or 200ft & backfilling complete | Rft | 100 |  |  |  |
| 10 | P/Laying precast RCC slab 2" thick include all cost of labour transportation with fixing of existing main hole etc. complete as directed by engineer incharge. | Sft | 20 |  |  |  |
| 11 | Vent pipe with cowel | Job | 2 |  |  |  |
| **C** | **Sign Board / Plaque** |  |  |  |  |  |
| 1 | Supply and installation of Sign Board / Branding sheet with organisation / Donors logos complete as per approved Design or as instructed by Engineer Incharge. | Job | 1 |  |  |  |
| **Sub-Total (IV)** | | | | |  | |

1. ***REPAIR AND RENOVATION MINOR WORK OF GD DOST MUHAMMAD HISBANI DISTRICT SHAHEED BENAZIRABAD, SIND PAKISTAN***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Sr. No.** | **Item Name** | **Unit** | **Quantity** | **Unit price of 1 item inclusive of taxes, packing, loading/ unloading, Transportation to Delivery Location of District Shaheed Benazirabad, Sindh**  **(To be filled in PKR by the bidder)** | **Total price inclusive of taxes, packing, loading/ unloading, Transportation to Delivery Location of District Shaheed Benazirabad, Sindh**  **(To be filled in PKR by the bidder)** | **Delivery Time in Days after PO/Supplies Contract**  **(To be filled in PKR by the bidder)** |
| **A** | **Civil Works** |  |  |  |  |  |
| 1 | Excavation in foundation of building, bridges, footpath, roads and other structure include dag, belling dressing refilling around structure with excavated earth watering and ramming lead up to 5ft etc. complete as directed by engineer in charge | Cft | 1668.50 |  |  |  |
| 2 | Dismantling cement concrete/ Brick work etc | Cft | 417.00 |  |  |  |
| 3 | Plain Cement Concrete including placing, compacting, finishing & curing (Ratio 1:4:8) | Cft | 391.17 |  |  |  |
| 4 | Pacca brick work in cement mortar in 1:6 ratio in Ground Floor as directed by Engineer In charge | Cft | 817.50 |  |  |  |
| 5 | Reinforced cement concrete work including all labour and material except the cost of steel reinforcement and its labour for bending and binding which will be paid separately. This rate also includes all kinds of forms moulds, lifting shuttering curing rendering and finishing the exposed surface (including screening and washing of shingle. (a)R.C work in roof slab, beams, columns rafts, lintels and other structural members laid in situ or precast laid in position complete in all respect.(I) Ratio 1:2:4 | Cft | 52.15 |  |  |  |
| 6 | Fabrication of mild steel reinforcement for cement concrete i/c cutting & bending and laying in position, making joints and fastenings including cost of binding wire(also includes removal of rust from bars) | KG | 115.94 |  |  |  |
| 7 | P/F GI Frame chowkhat Size 7"\*2" for Door using 20 gauge G.I Sheet I/C welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage, tools and plants using in making and fixing etc. complete. | Rft | 10.50 |  |  |  |
| 8 | Plain Cement Concrete including placing, compacting, finishing & curing (Ratio 1:2:4) | Cft | 311.57 |  |  |  |
| 9 | Removing cement or lime plaster | Sft | 2350.00 |  |  |  |
| 10 | Applying Floating coat of cement 1/32" thick | Sft | 2350.00 |  |  |  |
| 11 | Cement plaster 1:4 up to 20ft Heights & 1/2'' thick etc. complete | Sft | 4434.00 |  |  |  |
| 12 | Distempering three coat include scraping, Filling & Making surface smooth etc. complete as directed by engineer in charge. | Sft | 3520.06 |  |  |  |
| 13 | Preparing The Surface & painting with weather coat i/c rubbing the surface with rubbing brick / sand paper, filling the voids with chalk plaster of Paris & then painting weather coat of approved make. | Sft | 4911.16 |  |  |  |
| 14 | Painting of surface any type doors & window etc. complete in three coat. | Sft | 1481.60 |  |  |  |
| 15 | Cleaning of manholes, Septic Tank etc. | job | 1.00 |  |  |  |
| 16 | Cleaning of Latrine Bushes etc. | job | 1.00 |  |  |  |
| **B** | **PLUMBING WORK** |  |  |  |  |  |
| 1 | P/Fixing orise type white or colour glazed earthen ware WC Pan including P Trap & Complete with all other fixtures as directed by engineer incharge | No | 3 |  |  |  |
| 2 | P/Fixing 3 Gallon Flushing Cistern Complete with all fixtures as per instruction of Engineer incharge | No | 1 |  |  |  |
| 3 | Supplying/Fixing long bib cock of superior quality with c.p head 1/2' dia. (master, sonex,Porta brands). | No | 5 |  |  |  |
| 4 | Providing and fixing 1/2" and 3/4" dia UPVC pipe make Pak Arab include cutting, fitting including all fixtures etc complete as directed by engineer incharge. | Rft | 100 |  |  |  |
| 5 | P/Laying of RCC pipe 6" dia B class and digging trenches to required depth in fixing position including cutting, fixing, jointing & backfilling etc | Rft | 60 |  |  |  |
| 6 | Providing, laying UPVC pressure pipes of Class 'B'( equivalent make) digging trenches to required depth, fixing in trench i/c cutting, fitting and jointing with all fixers with 'Z' joint with one rubber ring i/c testing with water to a head 61 meter or 200ft & backfilling complete | Rft | 20 |  |  |  |
| 7 | P/Laying precast RCC slab 2" thick include all cost of labour transportation with fixing of existing main hole etc. complete as directed by engineer incharge. | Sft | 20 |  |  |  |
| 8 | Providing and fixing of water pump Set 1 hp set 2800 PRM single phase 220 volts 1-1/4x1" suction and delivery 40 ft head including base plate and also making C.C 1:3:6 plate form of required size and fixing with nuts and both complete in all respect.(R.A) | No | 1 |  |  |  |
|  | Vent pipe with cowel | Job | 2 |  |  |  |
| **C** | **Sign Board / Plaque** |  |  |  |  |  |
| 1 | Supply and installation of Sign Board / Branding sheet with organisation / Donors logos complete as per approved Design or as instructed by Engineer Incharge. | Job | 1 |  |  |  |
| **Sub-Total (V)** | | | | |  | |

1. ***REPAIR AND RENOVATION MINOR WORK OF GD GAWAR MAHAR DISTRICT SHAHEED BENAZIRABAD, SIND PAKISTAN***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Sr. No.** | **Item Name** | **Unit** | **Quantity** | **Unit price of 1 item inclusive of taxes, packing, loading/ unloading, Transportation to Delivery Location of District Shaheed Benazirabad, Sindh**  **(To be filled in PKR by the bidder)** | **Total price inclusive of taxes, packing, loading/ unloading, Transportation to Delivery Location of District Shaheed Benazirabad, Sindh**  **(To be filled in PKR by the bidder)** | **Delivery Time in Days after PO/Supplies Contract**  **(To be filled in PKR by the bidder)** |
| **A** | **Civil Works** |  |  |  |  |  |
| 1 | Excavation in foundation of building, bridges, footpath, roads and other structure include dag, belling dressing refilling around structure with excavated earth watering and ramming lead up to 5ft etc. complete as directed by engineer in charge | Cft | 275.00 |  |  |  |
| 2 | Dismantling cement concrete/ Brick work etc | Cft | 150.00 |  |  |  |
| 3 | Plain Cement Concrete including placing, compacting, finishing & curing (Ratio 1:4:8) | Cft | 34.56 |  |  |  |
| 4 | Pacca brick work in cement mortar in 1:6 ratio in Ground Floor as directed by Engineer In charge | Cft | 723.75 |  |  |  |
| 5 | Reinforced cement concrete work including all labour and material except the cost of steel reinforcement and its labour for bending and binding which will be paid separately. This rate also includes all kinds of forms moulds, lifting shuttering curing rendering and finishing the exposed surface (including screening and washing of shingle. (a)R.C work in roof slab, beams, columns rafts, lintels and other structural members laid in situ or precast laid in position complete in all respect.(I) Ratio 1:2:4 | Cft | 29.38 |  |  |  |
| 6 | Fabrication of mild steel reinforcement for cement concrete i/c cutting & bending and laying in position, making joints and fastenings including cost of binding wire(also includes removal of rust from bars) | KG | 65.31 |  |  |  |
| 7 | P/F GI Frame chowkhat Size 7"\*2" for Door using 20 gauge G.I Sheet I/C welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage, tools and plants using in making and fixing etc. complete. | Rft | 49.25 |  |  |  |
| 8 | Plain Cement Concrete including placing, compacting, finishing & curing (Ratio 1:2:4) | Cft | 264.99 |  |  |  |
| 9 | Removing cement or lime plaster | Sft | 974.43 |  |  |  |
| 10 | Applying Floating coat of cement 1/32" thick | Sft | 974.43 |  |  |  |
| 11 | Cement plaster 1:4 up to 20ft Heights & 1/2'' thick etc. complete | Sft | 2122.43 |  |  |  |
| 12 | Distempering three coat include scraping, Filling & Making surface smooth etc. complete as directed by engineer in charge. | Sft | 3854.08 |  |  |  |
| 13 | Preparing The Surface & painting with weather coat i/c rubbing the surface with rubbing brick / sand paper, filling the voids with chalk plaster of Paris & then painting weather coat of approved make. | Sft | 5997.91 |  |  |  |
| 14 | Painting of surface any type doors & window etc. complete in three coat. | Sft | 1150.00 |  |  |  |
| 15 | Providing and fixing in position doors, windows and ventilators of 1st class deodar wood frames and 1-1/2" thick teak wood ply shutters of 2nd class deodar wood skeleton (Solid) styles and rails core of partial wood and teak ply wood (3-ply) on both sides i/c holds fasts, hinges, iron tower bolts, handles and cleats with cord etc complete | Sft | 1.00 |  |  |  |
| 16 | Repair of Main Gate including welding, locks & increasing height etc complete | job | 1.00 |  |  |  |
| 17 | Installation of Wire gauze including all fixers as instructed by engineer incharge | Sft | 209.00 |  |  |  |
| 18 | Cleaning of manholes, Septic Tank, Bushes etc. | job | 1.00 |  |  |  |
| 19 | Cleaning of Latrine & Bushes etc. | job | 1.00 |  |  |  |
| 20 | Roof cleaning two coat cementation German acrylic chemical cracke filling and bandage laying of canvas cloth 4 Onz entire roof then apply two coat cementation German acrylic chemical, finally apply one coat Everseal. | Sft | 774.82 |  |  |  |
| **B** | **PLUMBING WORK** |  |  |  |  |  |
| 1 | P/Fixing orise type white or colour glazed earthen ware WC Pan including P Trap & Complete with all other fixtures as directed by engineer incharge | No | 1 |  |  |  |
| 2 | Supplying/Fixing long bib cock of superior quality with c.p head 1/2' dia. (master, sonex,Porta brands). | No | 2 |  |  |  |
| 3 | Supplying & Fixing fibre glass tank of approved quality and design and wall thickness as specified I/c cost of nuts, bolts and fixing in plateform of cement concrete 1:3:6 and making connections for in-let, & out-let & over flow pipes etc. complete 350 gallons wall thickness 3.5mm | No | 1 |  |  |  |
| 4 | Providing and fixing 1/2" and 3/4" dia UPVC pipe make Pak Arab include cutting, fitting including all fixtures etc complete as directed by engineer incharge. | Rft | 150 |  |  |  |
| 5 | Providing, laying UPVC pressure pipes of Class 'B'( equivalent make) digging trenches to required depth, fixing in trench i/c cutting, fitting and jointing with all fixers with 'Z' joint with one rubber ring i/c testing with water to a head 61 meter or 200ft & backfilling complete | Rft | 210 |  |  |  |
| 6 | P/Laying precast RCC slab 2" thick include all cost of labour transportation with fixing of existing main hole etc. complete as directed by engineer incharge. | Sft | 20 |  |  |  |
| 7 | Providing and fixing of water pump Set 1 hp set 2800 PRM single phase 220 volts 1-1/4x1" suction and delivery 40 ft head including base plate and also making C.C 1:3:6 plate form of required size and fixing with nuts and both complete in all respect.(R.A) | No | 1 |  |  |  |
| 8 | Vent pipe with cowel | Job | 1 |  |  |  |
| **C** | **Sign Board / Plaque** |  |  |  |  |  |
| 1 | Supply and installation of Sign Board / Branding sheet with organisation / Donors logos complete as per approved Design or as instructed by Engineer Incharge. | Job | 1 |  |  |  |
| **Sub-Total (VI)** | | | | |  | |

1. ***REPAIR AND RENOVATION MINOR WORK OF GD USMAN LAKHO DISTRICT SHAHEED BENAZIRABAD, SIND PAKISTAN***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Sr. No.** | **Item Name** | **Unit** | **Quantity** | **Unit price of 1 item inclusive of taxes, packing, loading/ unloading, Transportation to Delivery Location of District Shaheed Benazirabad, Sindh**  **(To be filled in PKR by the bidder)** | **Total price inclusive of taxes, packing, loading/ unloading, Transportation to Delivery Location of District Shaheed Benazirabad, Sindh**  **(To be filled in PKR by the bidder)** | **Delivery Time in Days after PO/Supplies Contract**  **(To be filled in PKR by the bidder)** |
| **A** | **Civil Works** |  |  |  |  |  |
| 1 | Excavation in foundation of building, bridges, footpath, roads and other structure include dag, belling dressing refilling around structure with excavated earth watering and ramming lead up to 5ft etc. complete as directed by engineer in charge | Cft | 230.00 |  |  |  |
| 2 | Dismantling cement concrete/ Brick work etc | Cft | 512.00 |  |  |  |
| 3 | Plain Cement Concrete including placing, compacting, finishing & curing (Ratio 1:4:8) | Cft | 331.93 |  |  |  |
| 4 | Pacca brick work in cement mortar in 1:6 ratio in Ground Floor as directed by Engineer In charge | Cft | 184.38 |  |  |  |
| 5 | Reinforced cement concrete work including all labour and material except the cost of steel reinforcement and its labour for bending and binding which will be paid separately. This rate also includes all kinds of forms moulds, lifting shuttering curing rendering and finishing the exposed surface (including screening and washing of shingle. (a)R.C work in roof slab, beams, columns rafts, lintels and other structural members laid in situ or precast laid in position complete in all respect.(I) Ratio 1:2:4 | Cft | 13.38 |  |  |  |
| 6 | Fabrication of mild steel reinforcement for cement concrete i/c cutting & bending and laying in position, making joints and fastenings including cost of binding wire(also includes removal of rust from bars) | KG | 29.74 |  |  |  |
| 7 | P/F GI Frame chowkhat Size 7"\*2" for Door using 20 gauge G.I Sheet I/C welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage, tools and plants using in making and fixing etc. complete. | Rft | 24.00 |  |  |  |
| 8 | Plain Cement Concrete including placing, compacting, finishing & curing (Ratio 1:2:4) | Cft | 143.44 |  |  |  |
| 9 | Removing cement or lime plaster | Sft | 1642.02 |  |  |  |
| 10 | Applying Floating coat of cement 1/32" thick | Sft | 1642.02 |  |  |  |
| 11 | Cement plaster 1:4 up to 20ft Heights & 1/2'' thick etc. complete | Sft | 1642.02 |  |  |  |
| 12 | Distempering three coat include scraping, Filling & Making surface smooth etc. complete as directed by engineer in charge. | Sft | 3607.56 |  |  |  |
| 13 | Preparing The Surface & painting with weather coat i/c rubbing the surface with rubbing brick / sand paper, filling the voids with chalk plaster of Paris & then painting weather coat of approved make. | Sft | 4541.16 |  |  |  |
| 14 | Painting of surface any type doors & window etc. complete in three coat. | Sft | 1394.10 |  |  |  |
| 15 | Installation of Wire gauze including all fixers as instructed by engineer incharge | Sft | 299.80 |  |  |  |
| 16 | Cleaning of manholes, Septic Tank etc. | job | 1.00 |  |  |  |
| 17 | Cleaning of Latrine & Bushes Etc | job | 1.00 |  |  |  |
| 18 | Roof cleaning two coat cementation German acrylic chemical cracke filling and bandage laying of canvas cloth 4 Onz entire roof then apply two coat cementation German acrylic chemical, finally apply one coat Everseal. | Sft | 283.35 |  |  |  |
| **B** | **PLUMBING WORK** |  |  |  |  |  |
| 1 | P/Fixing orise type white or colour glazed earthen ware WC Pan including P Trap & Complete with all other fixtures as directed by engineer incharge | No | 1 |  |  |  |
| 2 | P/Fixing 3 Gallon Flushing Cistern Complete with all fixtures as per instruction of Engineer incharge | No | 1 |  |  |  |
| 3 | Supplying/Fixing long bib cock of superior quality with c.p head 1/2' dia. (master, sonex,Porta brands). | No | 4 |  |  |  |
| 4 | Providing and fixing 1/2" and 3/4" dia UPVC pipe make Pak Arab include cutting, fitting including all fixtures etc complete as directed by engineer incharge. | Rft | 150 |  |  |  |
| 5 | P/Laying of RCC pipe 6" dia B class and digging trenches to required depth in fixing position including cutting, fixing, jointing & backfilling etc | Rft | 66 |  |  |  |
| 6 | Providing, laying UPVC pressure pipes of Class 'B'( equivalent make) digging trenches to required depth, fixing in trench i/c cutting, fitting and jointing with all fixers with 'Z' joint with one rubber ring i/c testing with water to a head 61 meter or 200ft & backfilling complete | Rft | 20 |  |  |  |
| 7 | P/Laying precast RCC slab 2" thick include all cost of labour transportation with fixing of existing main hole etc. complete as directed by engineer incharge. | Sft | 20 |  |  |  |
| 8 | Vent pipe with cowel | Job | 2 |  |  |  |
| **C** | **Sign Board / Plaque** |  |  |  |  |  |
| 1 | Supply and installation of Sign Board / Branding sheet with organisation / Donors logos complete as per approved Design or as instructed by Engineer Incharge. | Job | 1 |  |  |  |
| **Sub-Total (VII)** | | | | |  | |

1. ***REPAIR AND RENOVATION MINOR WORK OF MCH SHAMIR ZARDARI DISTRICT SHAHEED***

***BENAZIRABAD, SINDH PAKISTAN***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Sr. No.** | **Item Name** | **Unit** | **Quantity** | **Unit price of 1 item inclusive of taxes, packing, loading/ unloading, Transportation to Delivery Location of District Shaheed Benazirabad, Sindh**  **(To be filled in PKR by the bidder)** | **Total price inclusive of taxes, packing, loading/ unloading, Transportation to Delivery Location of District Shaheed Benazirabad, Sindh**  **(To be filled in PKR by the bidder)** | **Delivery Time in Days after PO/Supplies Contract**  **(To be filled in PKR by the bidder)** |
| **A** | **Civil Works** |  |  |  |  |  |
| 1 | Dismantling cement concrete/ Brick work etc | Cft | 114.38 |  |  |  |
| 2 | Pacca brick work in cement mortar in 1:6 ratio in Ground Floor as directed by Engineer In charge | Cft | 55.34 |  |  |  |
| 3 | Reinforced cement concrete work including all labour and material except the cost of steel reinforcement and its labour for bending and binding which will be paid separately. This rate also includes all kinds of forms moulds, lifting shuttering curing rendering and finishing the exposed surface (including screening and washing of shingle. (a)R.C work in roof slab, beams, columns rafts, lintels and other structural members laid in situ or precast laid in position complete in all respect.(I) Ratio 1:2:4 | Cft | 45.81 |  |  |  |
| 4 | Fabrication of mild steel reinforcement for cement concrete i/c cutting & bending and laying in position, making joints and fastenings including cost of binding wire(also includes removal of rust from bars) | KG | 101.84 |  |  |  |
| 5 | P/F GI Frame chowkhat Size 7"\*2" for Door using 20 gauge G.I Sheet I/C welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage, tools and plants using in making and fixing etc. complete. | Rft | 1.13 |  |  |  |
| 6 | Removing cement or lime plaster | Sft | 1132.61 |  |  |  |
| 7 | Applying Floating coat of cement 1/32" thick | Sft | 1132.61 |  |  |  |
| 8 | Cement plaster 1:4 up to 20ft Heights & 1/2'' thick etc. complete | Sft | 1232.61 |  |  |  |
| 9 | Distempering three coat include scraping, Filling & Making surface smooth etc. complete as directed by engineer in charge. | Sft | 3854.08 |  |  |  |
| 10 | Preparing The Surface & painting with weather coat i/c rubbing the surface with rubbing brick / sand paper, filling the voids with chalk plaster of Paris & then painting weather coat of approved make. | Sft | 5997.91 |  |  |  |
| 11 | Painting of surface any type doors & window etc. complete in three coat. | Sft | 1006.00 |  |  |  |
| 12 | Cleaning of manholes, Septic Tank, Bushes etc. | job | 1.00 |  |  |  |
| 13 | Cleaning of Latrine, Bushes etc. | job | 1.00 |  |  |  |
| **B** | **PLUMBING WORK** |  |  |  |  |  |
| 1 | Supplying/Fixing long bib cock of superior quality with c.p head 1/2' dia. (master, sonex,Porta brands). | No | 2 |  |  |  |
| 2 | Providing and fixing 1/2" and 3/4" dia UPVC pipe make Pak Arab include cutting, fitting including all fixtures etc complete as directed by engineer incharge. | Rft | 100 |  |  |  |
| 3 | Providing, laying UPVC pressure pipes of Class 'B'( equivalent make) digging trenches to required depth, fixing in trench i/c cutting, fitting and jointing with all fixers with 'Z' joint with one rubber ring i/c testing with water to a head 61 meter or 200ft & backfilling complete | Rft | 80 |  |  |  |
| 4 | Vent pipe with cowel | Job | 2 |  |  |  |
| **C** | **Sign Board / Plaque** |  |  |  |  |  |
| 1 | Supply and installation of Sign Board / Branding sheet with organisation / Donors logos complete as per approved Design or as instructed by Engineer Incharge. | Job | 1 |  |  |  |
| **Sub-Total (VIII)** | | | | |  | |

1. ***REPAIR AND RENOVATION MINOR WORK OF GD TOTTI DISTRICT SHAHEED BENAZIRABAD, SINDH PAKISTAN***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Sr. No.** | **Item Name** | **Unit** | **Quantity** | **Unit price of 1 item inclusive of taxes, packing, loading/ unloading, Transportation to Delivery Location of District Shaheed Benazirabad, Sindh**  **(To be filled in PKR by the bidder)** | **Total price inclusive of taxes, packing, loading/ unloading, Transportation to Delivery Location of District Shaheed Benazirabad, Sindh**  **(To be filled in PKR by the bidder)** | **Delivery Time in Days after PO/Supplies Contract**  **(To be filled in PKR by the bidder)** |
| **A** | **Civil Works** |  |  |  |  |  |
| 1 | Reinforced cement concrete work including all labour and material except the cost of steel reinforcement and its labour for bending and binding which will be paid separately. This rate also includes all kinds of forms moulds, lifting shuttering curing rendering and finishing the exposed surface (including screening and washing of shingle. (a)R.C work in roof slab, beams, columns rafts, lintels and other structural members laid in situ or precast laid in position complete in all respect.(I) Ratio 1:2:4 | Cft | 3.00 |  |  |  |
| 2 | Fabrication of mild steel reinforcement for cement concrete i/c cutting & bending and laying in position, making joints and fastenings including cost of binding wire(also includes removal of rust from bars) | KG | 6.67 |  |  |  |
| 3 | P/F GI Frame chowkhat Size 7"\*2" for Door using 20 gauge G.I Sheet I/C welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage, tools and plants using in making and fixing etc. complete. | Rft | 16.00 |  |  |  |
| 4 | Plain Cement Concrete including placing, compacting, finishing & curing (Ratio 1:2:4) | Cft | 172.51 |  |  |  |
| 5 | Removing cement or lime plaster | Sft | 759.14 |  |  |  |
| 6 | Applying Floating coat of cement 1/32" thick | Sft | 759.14 |  |  |  |
| 7 | Cement plaster 1:4 up to 20ft Heights & 1/2'' thick etc. complete | Sft | 758.14 |  |  |  |
| 8 | Distempering three coat include scraping, Filling & Making surface smooth etc. complete as directed by engineer in charge. | Sft | 3520.06 |  |  |  |
| 9 | Preparing The Surface & painting with weather coat i/c rubbing the surface with rubbing brick / sand paper, filling the voids with chalk plaster of Paris & then painting weather coat of approved make. | Sft | 2871.16 |  |  |  |
| 10 | Painting of surface any type doors & window etc. complete in three coat. | Sft | 1481.60 |  |  |  |
| 11 | Providing and fixing in position doors, windows and ventilators of 1st class deodar wood frames and 1-1/2" thick teak wood ply shutters of 2nd class deodar wood skeleton (Solid) styles and rails core of partial wood and teak ply wood (3-ply) on both sides i/c holds fasts, hinges, iron tower bolts, handles and cleats with cord etc complete | Sft | 70.00 |  |  |  |
| 12 | Galvanized wire gauze 144 mesh per sqr. Inch of 22 S.W.G fixed two chokhats with 3/4" deodar strips and screws | Sft | 3.00 |  |  |  |
| 13 | Installation of Wire gauze including all fixers as instructed by engineer incharge | Sft | 299.80 |  |  |  |
| 14 | Cleaning of manholes, Septic Tank etc. | job | 1.00 |  |  |  |
| 15 | Cleaning of Latrine & Bushes etc. | job | 1.00 |  |  |  |
| **B** | **PLUMBING WORK** |  |  |  |  |  |
| 1 | P/Fixing 6"x2" x3" C.I floor trap of approved self cleaning design with a C.I screwed down gritting with or without a vent arm complete.(master, sonex,Porta brands) | No | 1 |  |  |  |
| 2 | P/Fixing 3 Gallon Flushing Cistern Complete with all fixtures as per instruction of Engineer incharge | No | 1 |  |  |  |
| 3 | S/Fixing of concealed stop cock of Superior quality with CP head 1/2" dia. (master brands) | No | 1 |  |  |  |
| 4 | Supplying/Fixing long bib cock of superior quality with c.p head 1/2' dia. (master, sonex,Porta brands). | No | 5 |  |  |  |
| 5 | Providing and fixing 1/2" and 3/4" dia UPVC pipe make Pak Arab include cutting, fitting including all fixtures etc complete as directed by engineer incharge. | Rft | 150 |  |  |  |
| 6 | Providing, laying UPVC pressure pipes of Class 'B'( equivalent make) digging trenches to required depth, fixing in trench i/c cutting, fitting and jointing with all fixers with 'Z' joint with one rubber ring i/c testing with water to a head 61 meter or 200ft & backfilling complete | Rft | 4 |  |  |  |
| 7 | P/Laying precast RCC slab 2" thick include all cost of labour transportation with fixing of existing main hole etc. complete as directed by engineer incharge. | Sft | 20 |  |  |  |
|  | Vent pipe with cowel | Job | 2 |  |  |  |
| **C** | **Sign Board / Plaque** |  |  |  |  |  |
| 1 | Supply and installation of Sign Board / Branding sheet with organisation / Donors logos complete as per approved Design or as instructed by Engineer Incharge. | Job | 1 |  |  |  |
| **Sub-Total (IX)** | | | | |  | |
| **GRAND TOTAL Sites ( I to IX)** | | | | |  | |

Grand Total Amount in words: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Name of Bidder Signature & Stamp of Bidder Date

Contact Number Email Address

Office Address