Doc 5c - Price Schedule

Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Tender Ref: OCT-23-128**

Please mention your bid / quote on this form along with your sign and stamp on each page or in the same manner on your letter head.

Delivery Location: Project area of District Shaheed Benazirabad, Sindh, Pakistan.

Lot No. 03 Construction/Rehabilitation of Climate Resilient Demo Latrines (Total 75 Sites)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Sr. No.** | **Item Name** | **Unit** | **Quantity** | **Unit price of 1 item inclusive of taxes, packing, loading/ unloading, Transportation to Delivery Location of District Shaheed Benazirabad, Sindh**  **(To be filled in PKR by the bidder)** | **Total price inclusive of taxes, packing, loading/ unloading, Transportation to Delivery Location of District Shaheed Benazirabad, Sindh**  **(To be filled in PKR by the bidder)** | **Delivery Time in Days after PO/Supplies Contract** |
| 1 | Plain Cement Concrete including placing, compacting, finishing & curing (Ratio 1:4:8) | CFT | 14.54 |  |  |  |
| 2 | 1st class brick work in Foundation, Super structure in Cement, sand mortar 1:6 | CFT | 222.08 |  |  |  |
| 3 | RCC in roof slab, beam, column & other structural members, insitu or precast. Type C (1:2:4) | CFT | 1.61 |  |  |  |
| 4 | Supply & fabricate M.S. reinforcement for cement concrete, (Hot rolled deformed bars Grade 40) | KG | 5.36 |  |  |  |
| 5 | Provide, lay, water & ram 4" thick clean coarse sand under floor / brick paving, complete | CFT | 10.00 |  |  |  |
| 6 | Plain Cement Concrete including placing, compacting, finishing & curing (Ratio 1:2:4) | CFT | 29.38 |  |  |  |
| 7 | Cement plaster 1:4 upto 20' height 1/2" thick | sft | 398.50 |  |  |  |
| 8 | Providing and fixing single leaf steel door with 1.5"x 1.5"x 1/8"angle iron frame fully panelled with M.S sheet 20 gauge (0.9mm pressed) painted with two coats of red oxide & 3 Coats of Dark Green paint with fitting of approved make including cost of fabrication, iron lugs, cutting holes and making good the damages to walls Complete | sft | 15.00 |  |  |  |
| 9 | Providing and Fixing glazed earthen ware WC squatting type with built-in foot rests, including P trap etc complete in all respects :White | No | 1.00 |  |  |  |
| 10 | Providing and Fixing PVC floor trap of approved quality including grating, Jali, Outlet pipe & concrete chamber all round : 4"x2" (100mm x 50 mm) | Job | 1.00 |  |  |  |
| 11 | P/L approved quality UPVC pipes for water supply and gas supply i/c fitting, cutting, jointing, jointing material making holes in walls and filling the same with 1:4 CSM, excavation and back filling. : 4" dia | Ft | 14.00 |  |  |  |
| 12 | P/F approved quality UPVC Vent pipes 2" complete including Cowl & Complete fittings. | Job | 1.00 |  |  |  |
| 13 | Pre-Cast RCC slabs having size bracing thickness 2'', centre thickness 3/4'' Complete inclduing Girders for support & grouting above slabs | sft | 71.75 |  |  |  |
| 14 | Mild Steel Hand rail on both side,Stair/Ramp 2.5' height 1.5" x1.5" Square (450 gm/ft) including concrete etc complete | Job | 1.00 |  |  |  |
| 15 | Visibility Plates/ Inauguration Plaque as instructed by Engineer incharge | Job | 1.00 |  |  |  |
| 16 | Provision of Steel Folding Commode Chair with adjustable height for Elder/disable persons | Job | 1.00 |  |  |  |
| **TOTAL AMOUNT for 01 Latrine** | | | | |  | |
| **TOTAL AMOUNT for 75 Latrines** | | | | |  | |

Grand Total Amount in words: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Name of Bidder Signature & Stamp of Bidder Date

Contact Number Email Address

Office Address