Doc 5 - Price Schedule

Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Tender Ref: OCT-23-130 (Medical Equipment)**

Please mention your bid / quote on this form along with your sign and stamp on each page or in the same manner on your letter head.

Delivery Location: Project area of District Shaheed Benazirabad, Sindh.

Lot No. 01: Provision of Medical Equipment

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Sr. No.** | **Item Name** | **Item Specification** | **Unit** | **Quantity** | **Unit price of 1 item inclusive of taxes, packing, loading/ unloading, Transportation to Delivery Locations of SHAHEED BENAZIRABAD**  **(To be filled in PKR by the bidder)** | **Total price inclusive of taxes, packing, loading/ unloading, Transportation to Delivery Locations of SHAHEED BENAZIRABAD**  **(To be filled in PKR by the bidder)** | **Delivery Time in Days after PO/Supplies Contract** |
| 1 | Ultrasound Machine | • Digital Portable Ultrasound Diagnostic Imaging System for gynaecology, obstetrics, abdominal, paediatric, small organ, vascular, urology, orthopaedics and nerve exams. System having DICOM Compatibility and upgradable to PW Doppler. • Display: 12” LCD/LED Monitor. • Probe: 2 – 5 MHz Multi Frequency Convex Probe. • Display Mode: B, B/B, 4B, B/M and M-Mode, B/C/D triplex mode, PW • Scanning Methods: Electronic Convex with extended view, Electronic Linear with trapezoid. • M-Mode: 6- Speeds more • Frequency Range: 2 – 10 MHz • Scanning Depth: 35cm or more • Frame Rate: 375 fps or more • Focusing: Adjustable  • TGC/STC: 8-Steps or more • Zoom: instant full screen view, Pan Zoom & spot zoom  • I/O Interfaces: Transducer Connector, 2-USB Ports, Ethernet Port, Video port. • Keyboard: Alphanumeric Keys with trackball & user defined keys.  • Cine Memory: 10000 frames or more. • System dynamic range: 200 db or more • Online UPS • Trapezoid Imaging, One touch auto optimization, Tissue Harmonic imaging, Built-in Imaging Tutorial as standard. • Local Made Trolley.  • Ultrasound Gel 5 litres • Sono Black & White thermal Printer. • Warranty 01 – year with parts and free service. | Nos. | 1 |  |  |  |
| 2 | Patient Bed | • Semi Fowler Bed • Single Crank Operation • Removeable Head  • Size: 3 x 6.5 feet • With Mattress Height 4 inches with rexine cover | Nos. | 09 |  |  |  |
| 3 | Autoclave (Vertical) | • Autoclave single drum (10" X 10") • Element 2000-watt copper made • Lead 100% copper wire • Material Stainless Steel • Chamber made of 1 piece without any welding • Power: Electric & Gas (both options) • Single Drum with stand | Nos. | 09 |  |  |  |
| 4 | Oxygen Cylinder 240 CFT | • Medical gas cylinder, portable, for oxygen, fitted with a valve and a pressure and flow regulator and stand • 240 CFT cylinder or 50 kg • Robust construction of steel trolley. • Powder-coated finish. • Complete with mask, ready to use, once cylinder is filled. | Nos. | 09 |  |  |  |
| 5 | Aneroid Sphygmomanometer (Wall Mounted BP Apparatus) | • Measurement range: 0-300mmHg • Accuracy: +/-3mmHg • Scale grading: 2mmHg • Packing: Box individual | Nos. | 09 |  |  |  |
| 6 | Glucometer | • Full automatic coding  • Test Strip Ejector • 100 Multi user ID capabality  • Test result in < 10 seconds • 1.5 ul blood sample • 365 test memory | Nos. | 09 |  |  |  |
| 7 | Pulse Oximeter | • Fingertip Pulse Oximeter • Battery-low indicator • Audible & visual alarm • Adjustable brightness  • Digital display • Good Accuracy | Nos. | 09 |  |  |  |
| 8 | Baby Warmer | • Pre-Warm Mode • Baby Temperature maintained • Horizontal Angle of the Warmer  Module can be adjusted  • With Stand | Nos. | 09 |  |  |  |
| 9 | Electronic Suction Machine | • Power Voltage: AC220V±22V,50Hz±1Hz • Max negative pressure: ≥0.09MPa • Noise:≤65dB (A) • Power:≤180VA • Pumping rate: ≥20L/min • Reservoir capacity: 2000 mL/pc, 2 pieces • Easy to carry, low noise, high negative pressure and large flux | Nos. | 09 |  |  |  |
| 10 | Vacuum Cup for Delivery | • Material Silicon • Adjustable with Suction Machine • Locally made | Nos. | 09 |  |  |  |
| 11 | Emergency Medicine Trolly | • Iron Material  • with Hood • Four Drawers with single lock • Trolly with 3-inch wheels • Two Cylinder holders  • Locally made good quality | Nos. | 09 |  |  |  |
| 12 | Nebulizer Machine | • Compressed air nebulization • Storage space for nebulization kit • Support for wide voltage input • Durable quality product • Non-slip body material • Power cord with fuse • Long tube | Nos. | 09 |  |  |  |
| 13 | Baby Weighing Scale (Digital) | • Large easy-to-read LCD display with a digit size of 23mm. • Non-slip rubber feet for safety • Easy-read digital display with weight shown in kg/lb/oz • Auto and manual hold function for wriggling babies | Nos. | 09 |  |  |  |
| 14 | Adult Weighing Scale (Analogue) | • Full Metal Body Design For Long Life • Weighing Capacity: 130 kg  • Easy To Read And Understand • Zero Adjustable Dial | Nos. | 09 |  |  |  |
| 15 | Normal Vaginal Delivery (NVD) Kit | • Kidney Tray, 02 Straight Clamps, Cord Cutting Scissor, Sponge Holding Forcep,   Plain Scissor and Instrument Tray.  • Stainless Steel Instruments • Rust Free Instruments | Nos. | 09 |  |  |  |
| 16 | Normal Vaginal Delivery (NVD) Table | • Foldable leg section • High-quality 4" Foam with rexine cover • Head section has step-less adjustment using friction lock • Stainless Steel collection bowl supplied with a couch • Epoxy powder-coated finish  • Size 2 x 6 feet • 18 Guage Pipe | Nos. | 09 |  |  |  |
| 17 | PV Examination Light | • LEDs Light • Flexible Swan Neck • Stand with wheels | Nos. | 09 |  |  |  |
| 18 | Penguin Suction Bulb | • Silicon Suction Bulb • Autoclavable and reusable • Fluid Capacity 75 to 100 ML | Nos. | 18 |  |  |  |
| 19 | Foot Step | • Double Foot Step with Ruber Boots • Powder Coated finish • Color White • Two Steps | Nos. | 18 |  |  |  |
| **Total Amount** | | | | | |  | |

Grand Total Amount in words: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Name of Bidder Signature & Stamp of Bidder Date

Contact Number Email Address

Office Address