Doc 5c - Price Schedule

Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Tender Ref: AUG-24-135**

Please mention your bid / quote on this form along with your sign and stamp on each page or in the same manner on your letter head.

Delivery Location: Project area of District Dadu, Badin & Matiari, Sindh.

Lot No. 03: *REHAB OF LATRINES IN COMMUNITY, SCHOOLS & HEALTH FACILITIES (120 Latrines)*

Rehabilitation of Climate Resilient Latrines in Govt. Schools & Health Facilities (120 Latrines)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **S.No** | **Item Specification** | **Quantity Per Kit** | **Unit** | **Unit price of 1 item inclusive of taxes, packing, loading/ unloading, Transportation to Delivery Locations of Dadu, Badin & Matiari, Sindh**  **(To be filled in PKR by the bidder)** | **Total price inclusive of taxes, packing, loading/ unloading, Transportation to Delivery Locations of Dadu, Badin & Matiari, Sindh**  **(To be filled in PKR by the bidder)** | **Delivery Time in Days after PO/Supplies Contract** |
| 1 | Dismantling of concrete, brick work etc. | 63.00 | CFT |  |  |  |
| 2 | Cleaning work etc. | 1.00 | Job |  |  |  |
| 3 | Excavation in foundation of building, bridges etc. complete in ordinary soil | 227.00 | CFT |  |  |  |
| 4 | Plain Cement Concrete including placing, compacting, finishing & curing (Ratio 1:4:8) | 14.54 | CFT |  |  |  |
| 5 | 1st class brick work in Foundation, Super structure in Cement, sand mortar 1:6 | 237.83 | CFT |  |  |  |
| 6 | RCC in roof slab, beam, column & other structural members, insitu or precast. Type C (1:2:4) | 1.61 | CFT |  |  |  |
| 7 | Supply & fabricate M.S. reinforcement for cement concrete, (Hot rolled deformed bars Grade 40) | 5.36 | KG |  |  |  |
| 8 | Filling, watering and ramming earth under floor with earth excavated from outside lead upto 30m | 80.00 | CFT |  |  |  |
| 9 | Provide, lay, water & ram 4" thick clean coarse sand under floor / brick paving, complete | 10.00 | CFT |  |  |  |
| 10 | Plain Cement Concrete including placing, compacting, finishing & curing (Ratio 1:2:4) | 29.38 | CFT |  |  |  |
| 11 | Removing cement or lime plaster | 10.00 | sft |  |  |  |
| 12 | Applying Floating coat of cement 1/32" thick | 10.00 | sft |  |  |  |
| 13 | Cement plaster 1:4 upto 20' height 1/2" thick | 440.50 | sft |  |  |  |
| 14 | Preparing the surface and painting with matt finishing include rubbing the surface filling the voids with zinc chalk plaster of Paris mixture applying first coat of premier making the surface and then painting 3 coats matt finish paint with ICI matt finish etc. | 144.00 | sft |  |  |  |
| 15 | Preparing The Surface & painting with Snowcem/ weather coat i/c rubbing the surface with rubbing brick / sand paper, filling the voids with chalk plaster of Paris & then painting weather coat of approved make | 240.00 | sft |  |  |  |
| 16 | laying floor of approved coloured glazed tiles 1/4" thick laid in white cement and pigment on a bed of 3/4" Thick cement motor 1:2 (as per need / Instructed by Engineer incharge) | 100.00 | sft |  |  |  |
| 17 | P/F GI Frame chowkhat Size 7"\*2" for Door using 20 gauge G.I Sheet I/C welded hinges and fixing at site with necessary hold fasts, filling with cement sand slurry of ratio 1:6 and repairing the jambs. The cost also i/c all carriage, tools and plants using in making and fixing etc. complete. (as per need / Instructed by Engineer incharge) | 16.50 | Rft |  |  |  |
| 18 | Providing and fixing in position doors, windows and ventilators of 1st class deodar wood frames and 1-1/2" thick teak wood ply shutters of 2nd class deodar wood skeleton (Solid) styles and rails core of partial wood and teak ply wood (3-ply) on both sides i/c holds fasts, hinges, iron tower bolts, handles and cleats with cord etc. with Wooden chowkat complete ((as per need / Instructed by Engineer incharge) | 15.00 | sft |  |  |  |
| 19 | Providing and fixing single leaf steel door with 1.5"x 1.5"x 1/8"angle iron frame fully panelled with M.S sheet 20 gauge (0.9mm pressed) painted with two coats of red oxide & 3 Coats of Dark Green paint with fitting of approved make including cost of fabrication, iron lugs, cutting holes and making good the damages to walls Complete (as per need / Instructed by Engineer incharge) | 15.00 | sft |  |  |  |
| 20 | Installation of Wire gauze including all fixers (as per need / Instructed by Engineer incharge) | 36.00 | sft |  |  |  |
| 21 | MS flat 1/2"x1/8" grill in windows of approved design including painting 3 coats & Wire gauze, complete ( as per need / Instructed by Engineer incharge) | 3.00 | sft |  |  |  |
| 22 | Providing and Fixing glazed earthen ware WC squatting type with built-in foot rests, including P trap etc complete in all respects :White | 1.00 | No |  |  |  |
| 23 | Providing and Fixing PVC floor trap of approved quality including grating, Jali, Outlet pipe & concrete chamber all round : 4"x2" (100mm x 50 mm) (as per need / Instructed by Engineer incharge) | 1.00 | Job |  |  |  |
| 24 | Providing and fixing 3/4" dia UPVC pipe Best quality include cutting etc. complete including all fixtures & fittings as directed by engineer incharge | 50.00 | Rft |  |  |  |
| 25 | Providing and fixing chromium plated (CP)bib-cock heavy duty of approved quality : 1.5 cm 1/2" | 1.00 | No |  |  |  |
| 26 | P/L approved quality UPVC pipes for water supply and gas supply i/c fitting, cutting, jointing, jointing material making holes in walls and filling the same with 1:4 CSM, excavation and back filling. : 4" dia | 14.00 | Ft |  |  |  |
| 27 | P/L approved quality RCC pipes for water supply and gas supply i/c fitting, cutting, jointing, jointing material including excavation and back filling. Complete : 6" dia | 14.00 | Ft |  |  |  |
| 28 | P/F approved quality UPVC Vent pipes 2" complete including Cowl & Complete fittings. (as per need / Instructed by Engineer incharge) | 1.00 | Job |  |  |  |
| 29 | Pre-Cast RCC slabs having size bracing thickness 2'', centre thickness 3/4'' Complete including Girders for support & grouting above slabs | 71.75 | sft |  |  |  |
| 30 | Mild Steel Hand rail on both side, Stair/Ramp 2.5' height 1.5" x1.5" Square (450 gm/ft) including concrete etc. complete (as per need / Instructed by Engineer incharge) | 1.00 | Job |  |  |  |
| 31 | Visibility Plates/ Inauguration Plaque Stainless steel ( 22 SWG) size 15"x12"as instructed by Engineer incharge | 1.00 | Job |  |  |  |
| 32 | Supplying & Fixing fiber glass tank of approved quality and design and wall thickness as specified I/c cost of nuts, bolts and fixing in platform of cement concrete 1:3:6 and making connections for in-let, & out-let & over flow pipes with gate valve etc. complete 100 gallons wall thickness 3.5mm (as per need / Instructed by Engineer incharge) | 1.00 | Job |  |  |  |
| 33 | Providing and Fixing glazed earthen ware wash hand basin (WHB/Venity) white in color of Porta or Bright, complete, size 56x40 cm (22"x16"), including pedestal, bracket set, Side Pillar Cook Water Tap, waste coupling, 1-1/4'' Ф strainers, 1-1/4'' Ф drain pipe, soap dish, complete in all respects: | 1.00 | Job |  |  |  |
| 34 | P/Fixing orise type white or colour glazed earthen ware European style Complete with all other fixtures as directed by engineer incharge | 1.00 | Job |  |  |  |
| 35 | P/Fixing Muslim Shower | 1.00 | Job |  |  |  |
| SUB TOTAL – ONE LATRINES SCHOOLS & HEALTH FACILITIES | | | |  | | |
| SUB TOTAL – (120) LATRINES SCHOOLS & HEALTH FACILITIES | | | |  | | |

Grand Total Amount in words: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Name of Bidder Signature & Stamp of Bidder Date

Contact Number Email Address

Office Address